Skip to main content
`Ctrl`+`K`
scipy.signal.

# cheb2ap

scipy.signal.cheb2ap(N, rs, *, xp=None, device=None)

  Return (z,p,k) for Nth-order Chebyshev type II analog lowpass filter.

  The returned filter prototype has attenuation of at least `rs` decibels in the stopband.

  The filter’s angular (e.g. rad/s) cutoff frequency is normalized to 1, defined as the point at which the attenuation first reaches `rs`.

  Parameters:
    N int

      The order of the filter

    rs float

      The attenuation in the stopband

    xp array_namespace, optional

      Optional array namespace. Should be compatible with the array API standard, or supported by array-api-compat. Default: `numpy`

    device any

      optional device specification for output. Should match one of the supported device specification in `xp`.

  Returns:
    z ndarray[complex128]

      Zeros of the transfer function.

    p ndarray[complex128]

      Poles of the transfer function.

    k float

      Gain of the transfer function.

  See also

  `cheby2`

    Filter design function using this prototype

  Notes

  Array API Standard Support

  `cheb2ap` has experimental support for Python Array API Standard compatible backends in addition to NumPy. Please consider testing these features by setting an environment variable `SCIPY_ARRAY_API=1` and providing CuPy, PyTorch, JAX, or Dask arrays as array arguments. The following combinations of backend and device (or other capability) are supported.

  Library | CPU | GPU
  --- | --- | ---
  NumPy | ✅ | n/a
  CuPy | n/a | ✅
  PyTorch | ✅ | ✅
  JAX | ✅ | ✅
  Dask | ✅ | n/a

  See Support for the array API standard for more information.