Skip to main content
`Ctrl`+`K`
scipy.signal.ShortTimeFFT.

# scipy.signal.ShortTimeFFT.p_min

property ShortTimeFFT.p_min

  The smallest possible slice index.

  `p_min` is the index of the left-most slice, where the window still sticks into the signal, i.e., has non-zero part for t >= 0. `k_min` is the smallest index where the window function of the slice `p_min` is non-zero.

  Since, per convention the zeroth slice is centered at t=0, `p_min` <= 0 always holds. A detailed example is provided in the Sliding Windows section of the SciPy User Guide.

  See also

  `k_min`

    The smallest possible signal index.

  `k_max`

    First sample index after signal end not touched by a time slice.

  `p_max`

    Index of first non-overlapping upper time slice.

  `p_num`

    Number of time slices, i.e., `p_max` - `p_min`.

  `p_range`

    Determine and validate slice index range.

  `ShortTimeFFT`

    Class this property belongs to.